<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="31.75" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="0" x2="59.69" y2="0" width="0" layer="20"/>
<wire x1="59.69" y1="0" x2="63.5" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="63.5" y1="3.81" x2="63.5" y2="31.75" width="0" layer="20"/>
<wire x1="63.5" y1="31.75" x2="59.69" y2="35.56" width="0" layer="20" curve="90"/>
<wire x1="59.69" y1="35.56" x2="3.81" y2="35.56" width="0" layer="20"/>
<wire x1="3.81" y1="35.56" x2="0" y2="31.75" width="0" layer="20" curve="90"/>
<text>IN</text>
<text>OUT</text>
<text>USB Power Injector rev A
 c  2018 Jetperch LLC</text>
<text>Data input
from host</text>
<text>USB output
to device</text>
<text>+</text>
<text>-</text>
<text>Host powered</text>
</plain>
<libraries>
<library name="jetperch">
<packages>
<package name="USB-B">
</package>
<package name="USB-A_RPCT">
</package>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="BANANA_JACK_6">
<description>&lt;h2&gt;Banana Jack&lt;/h2&gt;

Compatible with #6 hole size, such as Cinch 111-0703-001 (black) and 111-0702-01 (red).</description>
</package>
<package name="CONN_0.1_2X1_M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J3" library="jetperch" package="USB-B" value="1-1734346-1"/>
<element name="J4" library="jetperch" package="USB-A_RPCT" value="87583-3010RPALF"/>
<element name="H1" library="jetperch" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT"/>
<element name="H2" library="jetperch" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT"/>
<element name="H3" library="jetperch" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT"/>
<element name="H4" library="jetperch" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT"/>
<element name="J1" library="jetperch" package="BANANA_JACK_6" value="111-0702-001">
<attribute name="MPN" value="111-0702-001"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="J2" library="jetperch" package="BANANA_JACK_6" value="111-0703-001">
<attribute name="MPN" value="111-0703-001"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="J5" library="jetperch" package="BANANA_JACK_6" value="111-0702-001">
<attribute name="MPN" value="111-0702-001"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="J6" library="jetperch" package="BANANA_JACK_6" value="111-0703-001">
<attribute name="MPN" value="111-0703-001"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="J7" library="jetperch" package="CONN_0.1_2X1_M" value=""/>
</elements>
<signals>
<signal name="POS_IN">
<contactref element="J3" pad="1"/>
<contactref element="J5" pad="P$1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="POS_OUT">
<contactref element="J4" pad="1"/>
<contactref element="J1" pad="P$1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="SHIELD">
<contactref element="J3" pad="SHIELD@1"/>
<contactref element="J3" pad="SHIELD@2"/>
<contactref element="J4" pad="SHIELD@2"/>
<contactref element="J4" pad="SHIELD@1"/>
</signal>
<signal name="D_P">
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="D_N">
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J3" pad="4"/>
<contactref element="J6" pad="P$1"/>
<contactref element="J4" pad="4"/>
<contactref element="J2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
